1. Content table

[1. Content table 1](#_Toc30670111)

[2. Project Name: 2](#_Toc30670112)

[3. Document Status: 2](#_Toc30670113)

[4. Document History: 2](#_Toc30670114)

[5. Project Description: 2](#_Toc30670115)

[5.1 Project Functionalities: 2](#_Toc30670116)

[5.2 Block diagram: 3](#_Toc30670117)

[6. Speed control management: 3](#_Toc30670118)

1. Project Name: LED STRING ANIMATION\_PO5\_CYRS
2. Document Status: Draft

# Document History:


|  |  |  |  |
| --- | --- | --- | --- |
| Version | Author | Date | Change Description |
| 1.0 | Menna Mostafa | 23/1/2020 | Initial Creation for  Structure of strings of LEDs used to provide Tail and TI functions based on some input signals. |

# Project Description:

## Project Functionalities:

Strings of LEDS are used to provide Tail and TI functions based on some input signals.

## Block diagram:



# Speed control management:

Req \_ LED STRING ANIMATION\_PO5\_CYRS \_ 001 \_ v01 \_ Imp # HW&SW

{

At startup, **WELCOME** **mode** shall be one of the following modes:

First mode:

LEDS from L6 to L1 will be ON then from R1 to R6 will be ON

Then all LEDS will be OFF

Then from R6 to R1 will be ON then L1 to L6 will be ON

Then all LEDS will be off

Then all LEDS are ON and OFF

Second mode:

LEDS from R1 to R6 are ON LED by LED and at same time L1 to L6 are ON LED by LED

Then repeat this scenario again.

}

Req \_ LED STRING ANIMATION\_PO5\_CYRS \_ 002 \_ v01 \_ Imp # SW

{

When Tail switch is ON/OFF then Tail function will be activated.

}

Req \_ LED STRING ANIMATION\_PO5\_CYRS \_ 003 \_ v01 \_ Imp # SW

{

When TI switch is ON/OFF then TI function will be activated, LEDS from R1 to R6 or from L1 to L6 will be activated.

}