# 1. Project Name:

**PO5\_LED STRING ANIMATION**

# 2. Table History:

|  |  |  |  |
| --- | --- | --- | --- |
| **Author** | **Version** | **Date** | **Change Description** |
| Walid Adel | 1.0 | 23/1/2020 | Initial Creation |
| Youssef Kamal | 1.1 | 25/1/2020 | Changing Status section as mentioned in review sheet. |
| Walid Adel | 1.2 | 29/1/2020 | Added a Block diagram prototype, Microcontroller parametric and pins connections |
| Walid Adel | 1.3 | 4/2/2020 | Added requirement ID’s to the requirements, added list of tables, added PIN DIRECTION column to PINS Connection Table |

# 3. Document Status:

|  |  |  |  |
| --- | --- | --- | --- |
| **Author** | **Version** | **Date** | **Status** |
| **Walid Adel** | 1.3 | 4/2/2020 | Draft |

# 4. Table of Content:

Contents

[1. Project Name: 1](#_Toc31665843)

[2. Table History: 1](#_Toc31665844)

[3. Document Status: 1](#_Toc31665845)

[4. Table of Content: 1](#_Toc31665846)

[5. List of Tables 2](#_Toc31665847)

[6. Requirements: 2](#_Toc31665848)

[6.1 Block Diagram 2](#_Toc31665849)

[6.2 MICROCONTOLLER & PINS 3](#_Toc31665850)

# 5. List of Tables

[Microcontroller Parametric](#_Microcontroller_Parametric:) 3

[Microcontroller Brief Description](#_Microcontroller_Brief_Description:)  [3](#_Toc31664978)

[PINS Connection](#_PINS_Connection:) [4](#_Toc31664978)

# 6. Requirements:

Req\_PO5\_LSAN\_HSI\_001\_V01

Covers Req\_PO5\_LSAN\_CRS\_003\_V01

### 6.1 Block Diagram



Req\_PO5\_LSAN\_HSI\_002\_V01

Covers Req\_PO5\_LSAN\_CRS\_003\_V01

### 6.2 MICROCONTOLLER & PINS

#### Microcontroller Parametric:

|  |  |
| --- | --- |
| **Name** | **Value** |
| Program Memory Type | Flash |
| Program Memory Size (KB) | 32 |
| CPU Speed (MIPS/DMIPS) | 16 |
| SRAM (B) | 2048 |
| Data EEPROM/HEF (bytes) | 1024 |
| Digital Communication Peripherals | 1-UART, 1-SPI, 1-I2C |
| Capture/Compare/PWM Peripherals | 1 Input Capture, 1 CCP, 4PWM |
| Timers | 2 x 8-bit, 1 x 16-bit |
| Number of Comparators | 1 |
| Temperature Range (°C) | -40 to 85 |
| Operating Voltage Range (V) | 4.5 to 5.5V |
| Pin Count | 40 |

#### Microcontroller Brief Description:

|  |  |
| --- | --- |
| **Microcontroller Description** | The high-performance, low-power Microchip 8-bit AVR RISC-based microcontroller combines 32KB ISP flash memory with read-while-write capabilities, 1KB EEPROM, 2KB SRAM, 54/69 general purpose I/O lines, 32 general purpose working registers, a JTAG interface for boundary-scan and on-chip debugging/programming, three flexible timer/counters with compare modes, internal and external interrupts, serial programmable USART, a universal serial interface (USI) with start condition detector, an 8-channel 10-bit A/D converter, programmable watchdog timer with internal oscillator, SPI serial port, and five software selectable power saving modes. The device operates between 1.8-5.5 volts.  By executing powerful instructions in a single clock cycle, the device achieves throughputs approaching 1 MIPS per MHz, balancing power consumption and processing speed |

#### PINS Connection:

|  |  |  |  |
| --- | --- | --- | --- |
| **PIN NUMBER** | **PIN DESCRIPTION** | **PIN DIRECTION** | **CONNECTION** |
| 1 | PB0 | O/P | LED L\_TAIL\_1 |
| 2 | PB1 | O/P | LED L\_TAIL\_2 |
| 3 | PB2 | O/P | LED L\_TAIL\_3 |
| 4 | PB3 | O/P | LED L\_TAIL\_4 |
| 5 | PB4 | O/P | LED L\_TAIL\_5 |
| 6 | PB5 | O/P | LED L\_TAIL\_6 |
| 7 | PB6 | I/P | TRI STATE TI\_SWITCH |
| 8 | PB7 | I/P | TRI STATE TI\_SWITCH |
| 9 | RESET | N/A | Not Used |
| 10 | VCC | N/A | +5V |
| 11 | GND | N/A | 0V |
| 12 | XTAL2 | N/A | Not Used |
| 13 | XTAL1 | N/A | Not Used |
| 14 | PD0 | O/P | R\_TAIL\_1 |
| 15 | PD1 | O/P | R\_TAIL\_2 |
| 16 | PD2 | O/P | R\_TAIL\_3 |
| 17 | PD3 | O/P | R\_TAIL\_4 |
| 18 | PD4 | O/P | R\_TAIL\_5 |
| 19 | PD5 | O/P | R\_TAIL\_6 |
| 20 | PD6 | O/P with initial value = 0 | Not Used |
| 21 | PD7 | I/P | PUSH BUTTON TAIL\_PB |
| 22 | PC0 | O/P | LED R1 |
| 23 | PC1 | O/P | LED R2 |
| 24 | PC2 | O/P | LED R3 |
| 25 | PC3 | O/P | LED R4 |
| 26 | PC4 | O/P | LED R5 |
| 27 | PC5 | O/P | LED R6 |
| 28 | PC6 | O/P with initial value = 0 | Not Used |
| 29 | PC7 | O/P with initial value = 0 | Not Used |
| 30 | AVCC | N/A | Not Used |
| 31 | GND | N/A | 0V |
| 32 | AREF | N/A | Not Used |
| 33 | PA7 | O/P with initial value = 0 | Not Used |
| 34 | PA6 | O/P with initial value = 0 | Not Used |
| 35 | PA5 | O/P | LED L6 |
| 36 | PA4 | O/P | LED L5 |
| 37 | PA3 | O/P | LED L4 |
| 38 | PA2 | O/P | LED L3 |
| 39 | PA1 | O/P | LED L2 |
| 40 | PA0 | O/P | LED L1 |