LED String Animation

PO5\_LSAN

Youssef Muhammed Ahmed Kamal

Mennatullah Mostafa Abd El-Nabi

Walid Adel Hassan Saeed

Mohanad Fawzy Mohamed Ashour

Sarah Abdelrahman Ibrahim

**Software Requirements Specification Document**

Document status

|  |  |  |  |
| --- | --- | --- | --- |
| Version | Author | Date | Status |
| v.02 | Mohanad Sallam  Sarah AbdelRahman | 29/01/2020 | Draft |

Document history

|  |  |  |  |
| --- | --- | --- | --- |
| Version | Author | Date | Change description |
| v.01 | Mohanad Sallam | 23/1/2020 | Create initial draft |
| v.02 | Mohanad Sallam  Sarah AbdelRahman | 29/01/2020 | Adding requirements |

Contents

[1.0 Introduction 3](#_Toc30776696)

[1.1 Purpose 3](#_Toc30776697)

[1.2 Scope 3](#_Toc30776698)

[1.3 Definitions, Acronyms and Abbreviation 3](#_Toc30776699)

[1.4 References 3](#_Toc30776700)

[2.0 The Overall Description 4](#_Toc30776701)

[2.1 User Needs 4](#_Toc30776702)

[2.2 Product perspective 4](#_Toc30776703)

[2.2.1 System interfaces 4](#_Toc30776704)

[2.2.2 Interfaces 4](#_Toc30776705)

[2.2.3 Communication Interfaces 4](#_Toc30776706)

[2.2.4 Memory constrains 4](#_Toc30776707)

[2.3 Assumptions and Dependencies 4](#_Toc30776708)

[3.0 Specific Requirements 4](#_Toc30776709)

[3.1 External Interfaces 4](#_Toc30776710)

[3.2 Functions 4](#_Toc30776711)

[3.3 System features 4](#_Toc30776712)

[3.4 Design Constraints 4](#_Toc30776713)

# Introduction

## Purpose

This is a v.02 of the requirements specifications for a LED String Animation.

## Scope

-Strings of LEDs as the following structure are used to provide Tail and TI functions based on some input signals.

- At startup, WELCOME mode shall be one of the following modes:

● **First mode:** LEDs shall be ON from L6 to L1, then from R1 to R6 and vice versa, and then all LEDs are ON and OFF.


● **Second mode:** LEDS from R1 to R6 are ON LED by LED and also the left branch at the same time, and then repeat the scenario again.

- Tail function shall be activated according to Tail switch.

- TI function shall be activated be activated according to TI switch, LEDs shall be activated LED by LED from R1 to R6 or from L1 to L6.

## Definitions, Acronyms and Abbreviation

## References



# 2.0 The Overall Description

## 2.1 User Needs

- Control the system through buttons

- Change the startup mode when needed

## 2.2 Product perspective

### 2.2.1 System interfaces

The system consists of 3 subsystems each has its own functionality:

1. Controls TI LEDs
2. Controls Tail LEDs
3. Sets the Startup mode

### 2.2.2 Interfaces

A unique signal is sent to the controller each controls one of the functionality.

### 2.2.3 Communication Interfaces

### 2.2.4 Memory constrains

## 2.3 Assumptions and Dependencies

# 3.0 Specific Requirements

**[Req \_ LED STRING ANIMATION\_PO5\_SRS \_ 001 \_ v01 ]**

(Req \_ LED STRING ANIMATION\_PO5\_CYRS \_ 001 \_ v01)

**[Req \_ LED STRING ANIMATION\_PO5\_SRS \_ 002 \_ v01]**

**[ A signal is sent to the controller to determine the status of the Tail LEDs**

**]** (Req \_ LED STRING ANIMATION\_PO5\_CYRS \_ 002 \_ v01)

**[Req \_ LED STRING ANIMATION\_PO5\_SRS \_ 003\_ v01]**

**[**A signal is sent from the controller to the Tails LEDs to indicate the activation or deactivation of them

**]** (Req \_ LED STRING ANIMATION\_PO5\_CYRS \_ 002 \_ v01)

**[Req \_ LED STRING ANIMATION\_PO5\_SRS \_ 004\_ v01]**

**[** A signal is sent to the controller to determine the status of the TI LEDs

**]** (Req \_ LED STRING ANIMATION\_PO5\_CYRS \_ 003 \_ v01 \_ Imp)

**[Req \_ LED STRING ANIMATION\_PO5\_SRS \_ 005\_ v01]**

[ A signal is

] (Req \_ LED STRING ANIMATION\_PO5\_CYRS \_ 003 \_ v01 \_ Imp)

## 3.1

## 3.2 Functions

## 3.3 System features

## 3.4 Design Constraints